int led = 13; // the pin the LED is connected to

void setup()

{

pinMode(led, OUTPUT) // Declare the LED as an output

}

void loop()

{

digitalWrite(led, HIGH) // Turn the LED on

}